Add a DMA channel for UART RX from the DMA tab